Master Switch On

☐ Interior and Exterior Lights

☐ Stall Warning Horn

☐ Pitot Heat

Walk Around

☐ Control Surfaces and Cables

☐ Drain Fuel Tank Sumps

* Remove all water and sediment; verify proper fuel.

☐ Drain Fuel Tank Strainer

* Move the selector OFF position, left, then right, while draining the strainer sump.

☐ Propeller

☐ Air Inlets and Alternator Belt Tension

☐ Oil Level (10-12 quarts)

☐ No Obvious Oil or Fuel Leaks

Landing Gear

☐ Strut Exposure (≥ 4.0″ / ≥ 2.6″)

☐ Visual Inspection of Tires

☐ Visual Inspection of Brake Blocks

Finishing Up

☐ Clean Windshield

☐ Prep Cockpit

☐ Engine Times and Stratus